**No load – 100V – Line to line voltage**

